This zip file contains the CTR2-MIDI.BIN firmware file that are used to flash the CTR2-MIDI firmware on to CTR2-MIDI hardware using the ESP32-S3 processor. This hardware supports both USB MIDI and Bluetooth-LE MIDI in CTR2-MIDI mode, and direct control of the Flex 6000/8000 radio in the Flex WiFi mode.

I've included the operation manuals for MIDI and WiFi modes. You can find configurations for many of the apps that CTR2-MIDI can be used with here: https://ctr2.lynovation.com/ctr2-midi-configuration-files/  

The operation manuals explain how to import these maps into your app. They are included in this zip file.

The operation files have been updated with the latest information on using the ESPConnect flash tool to update the firmware in you CTR2-MIDI.

The CTR2-MIDI_install.sh file is a script that you can use to install the firmware on your CTR2-MIDI without the need of the EspressIF Flash Download tool. This file is most useful on Linux and Mac PC. 

>>> If you use the script file remember to make it an executable file. <<<

To download these files to your device, extract them into a folder then use the instructions in Install or Update CTR2-MIDI Firmware section in the CTR2-MIDI or CTR2-MIDI_Flex_Mode operation manuals. 

73, Lynn, KU7Q